(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.531112)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" power)
    (2 "In2.Cu" power)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen") (color "White"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Red") (thickness 0.01524))
      (layer "F.Cu" (type "copper") (thickness 0.04572))
      (layer "dielectric 1" (type "prepreg") (thickness 0.178816) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.03048))
      (layer "dielectric 2" (type "core") (thickness 0.9906) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.03048))
      (layer "dielectric 3" (type "prepreg") (thickness 0.178816) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.04572))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Red") (thickness 0.01524))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen") (color "White"))
      (copper_finish "ENIG")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010e0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "fab/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+3V3")
  (net 3 "Net-(C10-Pad1)")
  (net 4 "Net-(C10-Pad2)")
  (net 5 "USB_3V3")
  (net 6 "Net-(C14-Pad1)")
  (net 7 "Net-(C15-Pad1)")
  (net 8 "Net-(C16-Pad1)")
  (net 9 "+5V_SW")
  (net 10 "MCLRn")
  (net 11 "PWM_OUT")
  (net 12 "Net-(C9-Pad2)")
  (net 13 "Net-(R6-Pad1)")
  (net 14 "Net-(R7-Pad1)")
  (net 15 "PWRENn")
  (net 16 "Net-(CR1-Pad2)")
  (net 17 "LOOPb")
  (net 18 "unconnected-(U4-Pad3)")
  (net 19 "LOOP_SENSE")
  (net 20 "unconnected-(U4-Pad6)")
  (net 21 "Net-(C20-Pad1)")
  (net 22 "unconnected-(U6-Pad4)")
  (net 23 "Net-(R13-Pad1)")
  (net 24 "WIFI_CSn")
  (net 25 "Net-(R14-Pad1)")
  (net 26 "WIFI_SPI_CLK")
  (net 27 "Net-(R15-Pad1)")
  (net 28 "WIFI_MOSI")
  (net 29 "Net-(R16-Pad1)")
  (net 30 "WIFI_MISO")
  (net 31 "Net-(U1-Pad22)")
  (net 32 "Net-(U1-Pad23)")
  (net 33 "Net-(U1-Pad24)")
  (net 34 "Net-(U1-Pad29)")
  (net 35 "Net-(U5-Pad6)")
  (net 36 "unconnected-(U3-Pad1)")
  (net 37 "U1CTSn")
  (net 38 "U1TX")
  (net 39 "unconnected-(U3-Pad5)")
  (net 40 "unconnected-(U3-Pad7)")
  (net 41 "unconnected-(U3-Pad8)")
  (net 42 "U1RTSn")
  (net 43 "unconnected-(U3-Pad10)")
  (net 44 "unconnected-(U3-Pad17)")
  (net 45 "unconnected-(U3-Pad18)")
  (net 46 "U1RX")
  (net 47 "Net-(C8-Pad1)")
  (net 48 "Net-(C11-Pad1)")
  (net 49 "Net-(K1-Pad1)")
  (net 50 "unconnected-(K1-Pad3)")
  (net 51 "unconnected-(K1-Pad5)")
  (net 52 "LOOPa")
  (net 53 "Net-(K2-Pad1)")
  (net 54 "unconnected-(K2-Pad3)")
  (net 55 "PTTb")
  (net 56 "unconnected-(K2-Pad5)")
  (net 57 "PTTa")
  (net 58 "PTT")
  (net 59 "AFSK_INa")
  (net 60 "unconnected-(T1-Pad2)")
  (net 61 "AFSK_INb")
  (net 62 "unconnected-(T1-Pad5)")
  (net 63 "Net-(T1-Pad6)")
  (net 64 "unconnected-(T2-Pad2)")
  (net 65 "AFSK_OUTb")
  (net 66 "unconnected-(T2-Pad5)")
  (net 67 "AFSK_OUTa")
  (net 68 "Net-(J1-Pad3)")
  (net 69 "Net-(J1-Pad4)")
  (net 70 "Net-(J1-Pad5)")
  (net 71 "Net-(J1-Pad6)")
  (net 72 "Net-(J1-Pad7)")
  (net 73 "PGED")
  (net 74 "PGEC")
  (net 75 "unconnected-(J2-Pad6)")
  (net 76 "unconnected-(J2-Pad7)")
  (net 77 "IDLEn")
  (net 78 "AUTOSTART")
  (net 79 "LOOP_KEY")
  (net 80 "Net-(R12-Pad2)")
  (net 81 "WIFI_EN")
  (net 82 "AFSK_OUT_ENn")
  (net 83 "unconnected-(U1-Pad33)")
  (net 84 "unconnected-(U1-Pad36)")
  (net 85 "unconnected-(U1-Pad37)")
  (net 86 "AUTOSTARTn")
  (net 87 "ENCODER_SWn")
  (net 88 "WIFI_IRQn")
  (net 89 "unconnected-(U1-Pad58)")
  (net 90 "WIFI_RESETn")
  (net 91 "unconnected-(U7-Pad1)")
  (net 92 "unconnected-(U7-Pad2)")
  (net 93 "unconnected-(U7-Pad3)")
  (net 94 "unconnected-(U7-Pad5)")
  (net 95 "unconnected-(U7-Pad6)")
  (net 96 "unconnected-(U7-Pad7)")
  (net 97 "unconnected-(U7-Pad8)")
  (net 98 "unconnected-(U7-Pad11)")
  (net 99 "unconnected-(U7-Pad14)")
  (net 100 "unconnected-(U7-Pad19)")
  (net 101 "unconnected-(U7-Pad21)")
  (net 102 "unconnected-(U7-Pad25)")
  (net 103 "unconnected-(U7-Pad26)")
  (net 104 "unconnected-(U7-Pad27)")
  (net 105 "KOS_LED")
  (net 106 "Net-(R22-Pad2)")
  (net 107 "TX_LED")
  (net 108 "Net-(R23-Pad2)")
  (net 109 "AUTOSTART_LED")
  (net 110 "Net-(R24-Pad2)")
  (net 111 "MOTOR_LED")
  (net 112 "Net-(R25-Pad2)")
  (net 113 "MARK_HI_LED")
  (net 114 "Net-(R26-Pad2)")
  (net 115 "850_SHIFT_LED")
  (net 116 "Net-(R27-Pad2)")
  (net 117 "SHIFT_TOGGLEn")
  (net 118 "KOS_TOGGLEn")
  (net 119 "TX_TOGGLEn")
  (net 120 "AUTOSTART_TOGGLEn")
  (net 121 "MOTOR_TOGGLEn")
  (net 122 "MARK_HI_TOGGLEn")
  (net 123 "QAn")
  (net 124 "QBn")
  (net 125 "+5V")
  (net 126 "unconnected-(S8-Pad1)")
  (net 127 "unconnected-(S8-Pad4)")
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.612 103.378 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "AUTOSTART_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Horizontal" (layer "F.Cu")
    (tedit 59FED5CB)
    (at 135.641 104.083 -90)
    (descr "Through hole angled pin header, 1x07, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 3.105 -2.535 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x07_Male" (at 4.385 17.51 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.77 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 134.112 101.346)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:BEADC2012X110N" (layer "F.Cu")
    (tedit 0)
    (at 165.608 55.968 -90)
    (descr "0805")
    (tags "Ferrite Bead")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Description" "Ferrite Beads 40ohms 100MHz 1.5A Monolithic 0805 SMD")
    (property "Height" "1.1")
    (property "Manufacturer_Name" "Laird Performance Materials")
    (property "Manufacturer_Part_Number" "MI0805K400R-10")
    (property "Mouser Part Number" "875-MI0805K400R-10")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Laird-Performance-Materials/MI0805K400R-10?qs=Hp4IEBVVqKKRJzYiDLfLSg%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at 3.468 1.524 90) (layer "F.SilkS"))
    (fp_text value "MI0805K400R-10" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.85 0 270) (size 1.2 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(C16-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0.85 0 270) (size 1.2 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "+5V") (pinfunction "2") (pintype "passive"))
    (model "MI0805K400R-10.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:UJ2-BH-BL1-TH" (layer "F.Cu")
    (tedit 641D1B1D)
    (at 170.18 52.07 180)
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -8.636 -1.016 180) (layer "F.SilkS"))
    (fp_text value "USB_B" (at 0.905395 15.692305) (layer "F.Fab"))
    (fp_text user "PCB EDGE" (at 5.04903 14.6863) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 8 "Net-(C16-Pad1)") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" thru_hole circle (at -2.5 0 180) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 7 "Net-(C15-Pad1)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -2.5 2 180) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 6 "Net-(C14-Pad1)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 0 2 180) (size 1.428 1.428) (drill 0.92) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "5" thru_hole circle (at -7.27 4.71 180) (size 3.316 3.316) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle (at 4.77 4.71 180) (size 3.316 3.316) (drill 2.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "SH") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.8 60.706)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "USB_3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "PWRENn") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:228DD1S1AAFAMSC" (layer "F.Cu")
    (tedit 0)
    (at 101.092 114.808 180)
    (descr "228DD1S1AAFAMSC")
    (tags "Switch")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.ctscorp.com/wp-content/uploads/228D.pdf")
    (property "Description" "SWITCH TACTILE SPST-NO 0.05A 12V")
    (property "Footprint_1" "228DD1S1AAFAMSC")
    (property "Height" "6.4")
    (property "Manufacturer_Name" "CTS")
    (property "Manufacturer_Part_Number" "228DD1S1AAFAMSC")
    (property "Mouser Part Number" "774-228DD1S1AAFAMSC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CTS-Electronic-Components/228DD1S1AAFAMSC?qs=BJlw7L4Cy7%252Bx9Gylbq7xIw%3D%3D")
    (property "Reference_1" "S?")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "228DD1S1AAFAMSC")
    (attr through_hole)
    (fp_text reference "S6" (at 1.725 4.572 180) (layer "F.SilkS"))
    (fp_text value "228DD1S1AAFAMSC" (at 1.725 -1.15 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.725 -1.15 180) (layer "F.Fab"))
    (pad "L1" thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 114 "Net-(R26-Pad2)") (pinfunction "A__AMBER") (pintype "passive"))
    (pad "L2" thru_hole circle (at 3.45 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K_AMBER") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 0.125 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 3.325 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH2") (pintype "passive"))
    (pad "S1" thru_hole circle (at 1.15 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 119 "TX_TOGGLEn") (pinfunction "COM") (pintype "passive"))
    (pad "S2" thru_hole circle (at 2.3 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "NO") (pintype "passive"))
  )
  (footprint "HhLibrary:74HCT2G14GWQ100H" (layer "F.Cu")
    (tedit 0)
    (at 178.308 65.786)
    (descr "74HCT2G14GW-Q100H")
    (tags "Integrated Circuit")
    (property "Arrow Part Number" "74HCT2G14GW-Q100H")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/74hct2g14gw-q100h/nexperia?region=nac")
    (property "Description" "Inverter IC 2 Channel Schmitt Trigger 6-TSSOP")
    (property "Height" "1.1")
    (property "Manufacturer_Name" "Nexperia")
    (property "Manufacturer_Part_Number" "74HCT2G14GW-Q100H")
    (property "Mouser Part Number" "771-74HCT2G14GWQ100H")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nexperia/74HCT2G14GW-Q100H?qs=fi7yB2oewZmNBzeOKw8f7A%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 3.44 -1.016) (layer "F.SilkS"))
    (fp_text value "74HCT2G14GW-Q100H" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.9 -0.75 90) (size 0.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "PWRENn") (pinfunction "1A") (pintype "passive"))
    (pad "2" smd rect (at -0.9 0 90) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect (at -0.9 0.75 90) (size 0.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "AUTOSTARTn") (pinfunction "2A") (pintype "passive"))
    (pad "4" smd rect (at 0.9 0.75 90) (size 0.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "AUTOSTART") (pinfunction "2Y") (pintype "passive"))
    (pad "5" smd rect (at 0.9 0 90) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "+5V_SW") (pinfunction "VCC") (pintype "passive"))
    (pad "6" smd rect (at 0.9 -0.75 90) (size 0.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "Net-(U5-Pad6)") (pinfunction "1Y") (pintype "passive"))
    (model "74HCT2G14GW-Q100H.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.526 82.042 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "33" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(R14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "WIFI_SPI_CLK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:228DD1S1AAFAMSC" (layer "F.Cu")
    (tedit 0)
    (at 90.932 114.808 180)
    (descr "228DD1S1AAFAMSC")
    (tags "Switch")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.ctscorp.com/wp-content/uploads/228D.pdf")
    (property "Description" "SWITCH TACTILE SPST-NO 0.05A 12V")
    (property "Footprint_1" "228DD1S1AAFAMSC")
    (property "Height" "6.4")
    (property "Manufacturer_Name" "CTS")
    (property "Manufacturer_Part_Number" "228DD1S1AAFAMSC")
    (property "Mouser Part Number" "774-228DD1S1AAFAMSC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CTS-Electronic-Components/228DD1S1AAFAMSC?qs=BJlw7L4Cy7%252Bx9Gylbq7xIw%3D%3D")
    (property "Reference_1" "S?")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "228DD1S1AAFAMSC")
    (attr through_hole)
    (fp_text reference "S5" (at 1.725 4.572 180) (layer "F.SilkS"))
    (fp_text value "228DD1S1AAFAMSC" (at 1.725 -1.15 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.725 -1.15 180) (layer "F.Fab"))
    (pad "L1" thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 112 "Net-(R25-Pad2)") (pinfunction "A__AMBER") (pintype "passive"))
    (pad "L2" thru_hole circle (at 3.45 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K_AMBER") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 0.125 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 3.325 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH2") (pintype "passive"))
    (pad "S1" thru_hole circle (at 1.15 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 118 "KOS_TOGGLEn") (pinfunction "COM") (pintype "passive"))
    (pad "S2" thru_hole circle (at 2.3 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "NO") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 59.944 75.184 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at -3.556 0 90) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "WIFI_EN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:1757569" (layer "F.Cu")
    (tedit 0)
    (at 148.283 48.196 180)
    (descr "1757569")
    (tags "Connector")
    (property "Arrow Part Number" "1757569")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/1757569/phoenix-contact")
    (property "Description" "PCB header, nominal cross section: 2.5 mm?, color: green, nominal current: 12 A, rated voltage (III/2): 320 V, contact surface: Tin, type of contact: Male connector, Number of potentials: 12, Number of rows: 1, Number of positions per row: 12, number of connections: 12, product range: MSTBA 2,5/..-G, pitch: 5 mm, mounting: Wave soldering, pin layout: Linear pinning, solder pin [P]: 3.5 mm, Stecksystem: CLASSIC COMBICON, Locking: without, type of packaging: packed in cardboard")
    (property "Height" "8.72")
    (property "Manufacturer_Name" "Phoenix Contact")
    (property "Manufacturer_Part_Number" "1757569")
    (property "Mouser Part Number" "651-1757569")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Phoenix-Contact/1757569?qs=A%2FKWGUWTCZjn%252BGnI2f1BNQ%3D%3D")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -5.133 -1.588 180) (layer "F.SilkS"))
    (fp_text value "1757569" (at 0 0 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 59 "AFSK_INa") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 61 "AFSK_INb") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 10 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 15 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 67 "AFSK_OUTa") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 20 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 65 "AFSK_OUTb") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at 25 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 57 "PTTa") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 30 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 55 "PTTb") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 35 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 78 "AUTOSTART") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 40 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 45 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 50 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 52 "LOOPa") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 55 0 180) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 "LOOPb") (pinfunction "12") (pintype "passive"))
    (model "1757569.stp"
      (offset (xyz -3.459999986 1.99999997 0.4999999925))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "Package_DIP:DIP-6_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 96.281 65.776 90)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K1" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "G3VM-601BY" (at 3.81 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(K1-Pad1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "unconnected-(K1-Pad3)") (pinfunction "3") (pintype "unspecified+no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "LOOPa") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "unconnected-(K1-Pad5)") (pinfunction "5") (pintype "unspecified+no_connect"))
    (pad "6" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(CR1-Pad2)") (pinfunction "6") (pintype "unspecified"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 140.97 82.042 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0.508 -3.048) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 80.772 103.378 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "MOTOR_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-6_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 107.696 66.04 90)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "K2" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "G3VM-601BY" (at 3.81 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(K2-Pad1)") (pinfunction "1") (pintype "unspecified"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "unconnected-(K2-Pad3)") (pinfunction "3") (pintype "unspecified+no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "PTTa") (pinfunction "4") (pintype "unspecified"))
    (pad "5" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "unconnected-(K2-Pad5)") (pinfunction "5") (pintype "unspecified+no_connect"))
    (pad "6" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "PTTb") (pinfunction "6") (pintype "unspecified"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.458 70.104 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "PTT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(K2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 127.254 76.2 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "100pF" (at 7.874 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.704 57.658 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 2.794 -0.254) (layer "F.SilkS"))
    (fp_text value "27" (at 5.334 -0.254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C15-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:ATWINC1510MR210UB" (layer "F.Cu")
    (tedit 0)
    (at 61.468 60.485 90)
    (descr "ATWINC15#0")
    (tags "Integrated Circuit")
    (property "Description" "WiFi Modules (802.11) SmartConnect ATWINC1500B-MU-T Module")
    (property "Height" "2.113")
    (property "Manufacturer_Name" "Microchip")
    (property "Manufacturer_Part_Number" "ATWINC1510-MR210UB")
    (property "Mouser Part Number" "556-ATWINC1510MR210U")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Microchip-Technology-Atmel/ATWINC1510-MR210UB?qs=QB0ovJDgFgt5QuIkS9qN8w%3D%3D")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 2.065 11.684 180) (layer "F.SilkS"))
    (fp_text value "ATWINC1510-MR210UB" (at -0.475 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -0.475 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -8.19 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "unconnected-(U7-Pad1)") (pinfunction "GPIO_6") (pintype "passive+no_connect"))
    (pad "2" smd rect (at -7.17 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "unconnected-(U7-Pad2)") (pinfunction "I2C_SCL") (pintype "passive+no_connect"))
    (pad "3" smd rect (at -6.154 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "unconnected-(U7-Pad3)") (pinfunction "I2C_SDA") (pintype "passive+no_connect"))
    (pad "4" smd rect (at -5.138 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "WIFI_RESETn") (pinfunction "RESET_N") (pintype "passive"))
    (pad "5" smd rect (at -1.074 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "unconnected-(U7-Pad5)") (pinfunction "NC_1") (pintype "passive+no_connect"))
    (pad "6" smd rect (at 0.958 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "unconnected-(U7-Pad6)") (pinfunction "NC_2") (pintype "passive+no_connect"))
    (pad "7" smd rect (at 1.974 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "unconnected-(U7-Pad7)") (pinfunction "NC_3") (pintype "passive+no_connect"))
    (pad "8" smd rect (at 2.99 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "unconnected-(U7-Pad8)") (pinfunction "NC_4") (pintype "passive+no_connect"))
    (pad "9" smd rect (at 4.006 7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "10" smd rect (at 1.974 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(R12-Pad2)") (pinfunction "SPI_CFG") (pintype "passive"))
    (pad "11" smd rect (at 0.958 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "unconnected-(U7-Pad11)") (pinfunction "WAKE") (pintype "passive+no_connect"))
    (pad "12" smd rect (at -0.058 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "13" smd rect (at -1.074 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "WIFI_IRQn") (pinfunction "IRQN") (pintype "passive"))
    (pad "14" smd rect (at -2.09 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "unconnected-(U7-Pad14)") (pinfunction "UART_TXD") (pintype "passive+no_connect"))
    (pad "15" smd rect (at -3.106 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "WIFI_MOSI") (pinfunction "SPI_MOSI") (pintype "passive"))
    (pad "16" smd rect (at -4.122 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "WIFI_CSn") (pinfunction "SPI_SSN") (pintype "passive"))
    (pad "17" smd rect (at -5.138 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R16-Pad1)") (pinfunction "SPI_MISO") (pintype "passive"))
    (pad "18" smd rect (at -6.154 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "WIFI_SPI_CLK") (pinfunction "SPI_SCK") (pintype "passive"))
    (pad "19" smd rect (at -7.17 -7.365 90) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "unconnected-(U7-Pad19)") (pinfunction "UART_RXD") (pintype "passive+no_connect"))
    (pad "20" smd rect (at -10.86 -5.465 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VBAT") (pintype "passive"))
    (pad "21" smd rect (at -10.86 -2.417 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U7-Pad21)") (pinfunction "GPIO_1") (pintype "passive+no_connect"))
    (pad "22" smd rect (at -10.86 -1.401 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "WIFI_EN") (pinfunction "CHIP_EN") (pintype "passive"))
    (pad "23" smd rect (at -10.86 -0.385 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDDIO") (pintype "passive"))
    (pad "24" smd rect (at -10.86 0.631 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(C20-Pad1)") (pinfunction "1P3V_TP") (pintype "passive"))
    (pad "25" smd rect (at -10.86 1.647 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "unconnected-(U7-Pad25)") (pinfunction "GPIO_3") (pintype "passive+no_connect"))
    (pad "26" smd rect (at -10.86 2.663 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "unconnected-(U7-Pad26)") (pinfunction "GPIO_4") (pintype "passive+no_connect"))
    (pad "27" smd rect (at -10.86 3.679 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U7-Pad27)") (pinfunction "GPIO_5") (pintype "passive+no_connect"))
    (pad "28" smd rect (at -10.86 4.695 180) (size 0.8 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND_3") (pintype "passive"))
    (model "ATWINC1510-MR210UB.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 130.302 93.726)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at -0.254 1.524) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:SOT95P280X145-6N" (layer "F.Cu")
    (tedit 0)
    (at 132.08 75.184)
    (descr "DBV0006A-")
    (tags "Integrated Circuit")
    (property "Arrow Part Number" "TLV2780CDBVT")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/tlv2780cdbvt/texas-instruments")
    (property "Description" "Operational Amplifiers - Op Amps Single 1.8V RRIO 8MHz")
    (property "Height" "1.45")
    (property "Manufacturer_Name" "Texas Instruments")
    (property "Manufacturer_Part_Number" "TLV2780CDBVT")
    (property "Mouser Part Number" "595-TLV2780CDBVT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TLV2780CDBVT?qs=m96fseALk3VixJMdPSjfFg%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.54) (layer "F.SilkS"))
    (fp_text value "TLV2780CDBVT" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 -0.95 90) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C10-Pad2)") (pinfunction "OUT") (pintype "passive"))
    (pad "2" smd rect (at -1.25 0 90) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect (at -1.25 0.95 90) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(C11-Pad1)") (pinfunction "IN+") (pintype "passive"))
    (pad "4" smd rect (at 1.25 0.95 90) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C10-Pad2)") (pinfunction "IN-") (pintype "passive"))
    (pad "5" smd rect (at 1.25 0 90) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "AFSK_OUT_ENn") (pinfunction "~{SHDN}") (pintype "passive"))
    (pad "6" smd rect (at 1.25 -0.95 90) (size 0.6 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDD") (pintype "passive"))
    (model "TLV2780CDBVT.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 56.134 75.184 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50.292 103.378 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at -3.302 0 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "MARK_HI_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(R27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.874 77.978 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 2.794 -0.254) (layer "F.SilkS"))
    (fp_text value "30k" (at -0.254 -1.524) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "PWM_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:DIPS1067W107P475L2062H1880Q6N" (layer "F.Cu")
    (tedit 0)
    (at 125.8055 67.818 90)
    (descr "DIP-6")
    (tags "Transformer")
    (property "Arrow Part Number" "TY-145P")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/ty-145p/triad-magnetics")
    (property "Description" "TRIAD MAGNETICS - TY-145P - TRANSFORMER, 1:1, 600/600")
    (property "Height" "18.796")
    (property "Manufacturer_Name" "Triad Magnetics")
    (property "Manufacturer_Part_Number" "TY-145P")
    (property "Mouser Part Number" "553-TY145P")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Triad-Magnetics/TY-145P?qs=sK90oOEhQaVS4WlcmrXXSA%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "T2" (at -4.826 -4.6475 180) (layer "F.SilkS"))
    (fp_text value "TY-145P" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 3 "Net-(C10-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.75 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 64 "unconnected-(T2-Pad2)") (pinfunction "2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 0 9.5 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at 10.668 9.5 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 67 "AFSK_OUTa") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.668 4.75 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 66 "unconnected-(T2-Pad5)") (pinfunction "5") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 10.668 0 90) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 65 "AFSK_OUTb") (pinfunction "6") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 136.652 74.168)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0.508 -1.524) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:228DD1S1AAFAMSC" (layer "F.Cu")
    (tedit 0)
    (at 50.292 114.808 180)
    (descr "228DD1S1AAFAMSC")
    (tags "Switch")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.ctscorp.com/wp-content/uploads/228D.pdf")
    (property "Description" "SWITCH TACTILE SPST-NO 0.05A 12V")
    (property "Footprint_1" "228DD1S1AAFAMSC")
    (property "Height" "6.4")
    (property "Manufacturer_Name" "CTS")
    (property "Manufacturer_Part_Number" "228DD1S1AAFAMSC")
    (property "Mouser Part Number" "774-228DD1S1AAFAMSC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CTS-Electronic-Components/228DD1S1AAFAMSC?qs=BJlw7L4Cy7%252Bx9Gylbq7xIw%3D%3D")
    (property "Reference_1" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "228DD1S1AAFAMSC")
    (attr through_hole)
    (fp_text reference "S1" (at 2.286 4.572 180) (layer "F.SilkS"))
    (fp_text value "228DD1S1AAFAMSC" (at 1.725 -1.15 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.725 -1.15 180) (layer "F.Fab"))
    (pad "L1" thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 116 "Net-(R27-Pad2)") (pinfunction "A__AMBER") (pintype "passive"))
    (pad "L2" thru_hole circle (at 3.45 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K_AMBER") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 0.125 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 3.325 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH2") (pintype "passive"))
    (pad "S1" thru_hole circle (at 1.15 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 122 "MARK_HI_TOGGLEn") (pinfunction "COM") (pintype "passive"))
    (pad "S2" thru_hole circle (at 2.3 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "NO") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 118.364 93.726 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C23" (at 0 1.524 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 177.8 62.484 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -4.064 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at -7.366 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "USB_3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 151.0295 94.234)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.748 82.042 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 3.302 0 90) (layer "F.SilkS"))
    (fp_text value "33" (at 5.588 -0.254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(R15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "WIFI_MOSI") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 127.254 72.644)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at -3.048 0) (layer "F.SilkS"))
    (fp_text value "1uF" (at -6.096 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 123.444 92.202)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U8" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "W25X40CLSN" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "Net-(U1-Pad24)") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(U1-Pad22)") (pinfunction "DO(IO1)") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "~{WP}") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "Net-(U1-Pad23)") (pinfunction "DI(IO0)") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "Net-(U1-Pad29)") (pinfunction "SCK") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "~{HOLD}") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 173.482 70.612 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+5V_SW") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:228DD1S1AAFAMSC" (layer "F.Cu")
    (tedit 0)
    (at 80.772 114.808 180)
    (descr "228DD1S1AAFAMSC")
    (tags "Switch")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.ctscorp.com/wp-content/uploads/228D.pdf")
    (property "Description" "SWITCH TACTILE SPST-NO 0.05A 12V")
    (property "Footprint_1" "228DD1S1AAFAMSC")
    (property "Height" "6.4")
    (property "Manufacturer_Name" "CTS")
    (property "Manufacturer_Part_Number" "228DD1S1AAFAMSC")
    (property "Mouser Part Number" "774-228DD1S1AAFAMSC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CTS-Electronic-Components/228DD1S1AAFAMSC?qs=BJlw7L4Cy7%252Bx9Gylbq7xIw%3D%3D")
    (property "Reference_1" "S?")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "228DD1S1AAFAMSC")
    (attr through_hole)
    (fp_text reference "S4" (at 1.725 4.572 180) (layer "F.SilkS"))
    (fp_text value "228DD1S1AAFAMSC" (at 1.725 -1.15 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.725 -1.15 180) (layer "F.Fab"))
    (pad "L1" thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 110 "Net-(R24-Pad2)") (pinfunction "A__AMBER") (pintype "passive"))
    (pad "L2" thru_hole circle (at 3.45 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K_AMBER") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 0.125 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 3.325 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH2") (pintype "passive"))
    (pad "S1" thru_hole circle (at 1.15 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 121 "MOTOR_TOGGLEn") (pinfunction "COM") (pintype "passive"))
    (pad "S2" thru_hole circle (at 2.3 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "NO") (pintype "passive"))
  )
  (footprint "HhLibrary:QFP50P1200X1200X120-64N" (layer "F.Cu")
    (tedit 0)
    (at 140.208 93.218 -90)
    (descr "64 LEAD TQFP*-")
    (tags "Integrated Circuit")
    (property "Arrow Part Number" "PIC32MZ0512EFE064-I/PT")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/pic32mz0512efe064-ipt/microchip-technology?region=nac")
    (property "Description" "Microchip PIC32MZ0512EFE064-I/PT, 32bit Microcontroller, 200MHz, 512 kB Flash, 64-Pin TQFP")
    (property "Height" "1.2")
    (property "Manufacturer_Name" "Microchip")
    (property "Manufacturer_Part_Number" "PIC32MZ0512EFE064-I/PT")
    (property "Mouser Part Number" "579-MZ0512EFE064IPT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Microchip-Technology/PIC32MZ0512EFE064-I-PT?qs=XR%2FfMt4sL%252BFV1SJpzPyuIA%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -5.842 -8.128 180) (layer "F.SilkS"))
    (fp_text value "PIC32MZ0512EFE064-I_PT" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -5.738 -3.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "LOOP_KEY") (pinfunction "AN17/ETXEN/RPE5/PMD5/RE5") (pintype "passive"))
    (pad "2" smd rect (at -5.738 -3.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "LOOP_SENSE") (pinfunction "AN16/ETXD0/PMD6/RE6") (pintype "passive"))
    (pad "3" smd rect (at -5.738 -2.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(R13-Pad1)") (pinfunction "AN15/ETXD1/PMD7/RE7") (pintype "passive"))
    (pad "4" smd rect (at -5.738 -2.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(R14-Pad1)") (pinfunction "AN14/C1IND/RPG6/SCK2/PMA5/RG6") (pintype "passive"))
    (pad "5" smd rect (at -5.738 -1.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "WIFI_MISO") (pinfunction "AN13/C1INC/RPG7/SDA4/PMA4/RG7") (pintype "passive"))
    (pad "6" smd rect (at -5.738 -1.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(R15-Pad1)") (pinfunction "AN12/C2IND/RPG8/SCL4/PMA3/RG8") (pintype "passive"))
    (pad "7" smd rect (at -5.738 -0.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_1") (pintype "passive"))
    (pad "8" smd rect (at -5.738 -0.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDD_1") (pintype "passive"))
    (pad "9" smd rect (at -5.738 0.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "MCLRn") (pinfunction "~{MCLR}") (pintype "passive"))
    (pad "10" smd rect (at -5.738 0.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "PWM_OUT") (pinfunction "AN11/C2INC/RPG9/PMA2/RG9") (pintype "passive"))
    (pad "11" smd rect (at -5.738 1.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "AFSK_OUT_ENn") (pinfunction "AN45/C1INA/RPB5/RB5") (pintype "passive"))
    (pad "12" smd rect (at -5.738 1.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "PTT") (pinfunction "AN4/C1INB/RB4") (pintype "passive"))
    (pad "13" smd rect (at -5.738 2.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "IDLEn") (pinfunction "AN3/C2INA/RPB3/RB3") (pintype "passive"))
    (pad "14" smd rect (at -5.738 2.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(T1-Pad6)") (pinfunction "AN2/C2INB/RPB2/RB2") (pintype "passive"))
    (pad "15" smd rect (at -5.738 3.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "PGEC") (pinfunction "PGEC1/VREF-/CVREF-/AN1/RPB1/RB1") (pintype "passive"))
    (pad "16" smd rect (at -5.738 3.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "PGED") (pinfunction "PGED1/VREF+/CVREF+/AN0/RPB0/PMA6/RB0") (pintype "passive"))
    (pad "17" smd rect (at -3.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "MARK_HI_TOGGLEn") (pinfunction "PGEC2/AN46/RPB6/RB6") (pintype "passive"))
    (pad "18" smd rect (at -3.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "MARK_HI_LED") (pinfunction "PGED2/AN47/RPB7/RB7") (pintype "passive"))
    (pad "19" smd rect (at -2.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "AVDD") (pintype "passive"))
    (pad "20" smd rect (at -2.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "AVSS") (pintype "passive"))
    (pad "21" smd rect (at -1.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 107 "TX_LED") (pinfunction "AN48/RPB8/PMA10/RB8") (pintype "passive"))
    (pad "22" smd rect (at -1.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(U1-Pad22)") (pinfunction "AN49/RPB9/PMA7/RB9") (pintype "passive"))
    (pad "23" smd rect (at -0.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "Net-(U1-Pad23)") (pinfunction "TMS/CVREFOUT/AN5/RPB10/PMA13/RB10") (pintype "passive"))
    (pad "24" smd rect (at -0.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "Net-(U1-Pad24)") (pinfunction "TDO/AN6/PMA12/RB11") (pintype "passive"))
    (pad "25" smd rect (at 0.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_2") (pintype "passive"))
    (pad "26" smd rect (at 0.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDD_2") (pintype "passive"))
    (pad "27" smd rect (at 1.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "SHIFT_TOGGLEn") (pinfunction "TCK/AN7/PMA11/RB12") (pintype "passive"))
    (pad "28" smd rect (at 1.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "850_SHIFT_LED") (pinfunction "TDI/AN8/RB13") (pintype "passive"))
    (pad "29" smd rect (at 2.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "Net-(U1-Pad29)") (pinfunction "AN9/RPB14/SCK3/PMA1/RB14") (pintype "passive"))
    (pad "30" smd rect (at 2.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "AUTOSTART_TOGGLEn") (pinfunction "AN10/EMDC/AEMDC/RPB15/OCFB/PMA0/RB15") (pintype "passive"))
    (pad "31" smd rect (at 3.25 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 121 "MOTOR_TOGGLEn") (pinfunction "OSC1/CLKI/RC12") (pintype "passive"))
    (pad "32" smd rect (at 3.75 5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "AUTOSTART_LED") (pinfunction "OSC2/CLKO/RC15") (pintype "passive"))
    (pad "33" smd rect (at 5.738 3.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "unconnected-(U1-Pad33)") (pinfunction "VBUS") (pintype "passive+no_connect"))
    (pad "34" smd rect (at 5.738 3.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VUSB3V3") (pintype "passive"))
    (pad "35" smd rect (at 5.738 2.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_3") (pintype "passive"))
    (pad "36" smd rect (at 5.738 2.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "unconnected-(U1-Pad36)") (pinfunction "D-") (pintype "passive+no_connect"))
    (pad "37" smd rect (at 5.738 1.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "unconnected-(U1-Pad37)") (pinfunction "D+") (pintype "passive+no_connect"))
    (pad "38" smd rect (at 5.738 1.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "U1RTSn") (pinfunction "RPF3/USBID/RF3") (pintype "passive"))
    (pad "39" smd rect (at 5.738 0.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDD_3") (pintype "passive"))
    (pad "40" smd rect (at 5.738 0.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_4") (pintype "passive"))
    (pad "41" smd rect (at 5.738 -0.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "U1RX") (pinfunction "RPF4/SDA5/PMA9/RF4") (pintype "passive"))
    (pad "42" smd rect (at 5.738 -0.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "U1TX") (pinfunction "RPF5/SCL5/PMA8/RF5") (pintype "passive"))
    (pad "43" smd rect (at 5.738 -1.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "U1CTSn") (pinfunction "AERXD0/ETXD2/RPD9/SDA1/PMCS2/PMA15/RD9") (pintype "passive"))
    (pad "44" smd rect (at 5.738 -1.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "AUTOSTARTn") (pinfunction "ECOL/RPD10/SCL1/SCK4/RD10") (pintype "passive"))
    (pad "45" smd rect (at 5.738 -2.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "TX_TOGGLEn") (pinfunction "AERXCLK/AEREFCLK/ECRS/RPD11/PMCS1/PMA14/RD11") (pintype "passive"))
    (pad "46" smd rect (at 5.738 -2.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(J1-Pad7)") (pinfunction "AERXD1/ETXD3/RPD0/RTCC/INT0/RD0") (pintype "passive"))
    (pad "47" smd rect (at 5.738 -3.25) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(J1-Pad6)") (pinfunction "SOSCI/RPC13/RC13") (pintype "passive"))
    (pad "48" smd rect (at 5.738 -3.75) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(J1-Pad5)") (pinfunction "SOSCO/RPC14/T1CK/RC14") (pintype "passive"))
    (pad "49" smd rect (at 3.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(J1-Pad4)") (pinfunction "EMDIO/AEMDIO/RPD1/SCK1/RD1") (pintype "passive"))
    (pad "50" smd rect (at 3.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(J1-Pad3)") (pinfunction "ETXERR/AETXEN/RPD2/SDA3/RD2") (pintype "passive"))
    (pad "51" smd rect (at 2.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "MOTOR_LED") (pinfunction "AERXERR/ETXCLK/RPD3/SCL3/RD3") (pintype "passive"))
    (pad "52" smd rect (at 2.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "KOS_TOGGLEn") (pinfunction "~{SQICS0}/RPD4/PMWR/RD4") (pintype "passive"))
    (pad "53" smd rect (at 1.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 105 "KOS_LED") (pinfunction "~{SQICS1}/RPD5/PMRD/RD5") (pintype "passive"))
    (pad "54" smd rect (at 1.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDD_4") (pintype "passive"))
    (pad "55" smd rect (at 0.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_5") (pintype "passive"))
    (pad "56" smd rect (at 0.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "ENCODER_SWn") (pinfunction "ERXD3/AETXD1/RPF0/RF0") (pintype "passive"))
    (pad "57" smd rect (at -0.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "WIFI_IRQn") (pinfunction "TRCLK/SQICLK/ERXD2/AETXD0/RPF1/RF1") (pintype "passive"))
    (pad "58" smd rect (at -0.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "unconnected-(U1-Pad58)") (pinfunction "TRD0/SQID0/ERXD1/PMD0/RE0") (pintype "passive+no_connect"))
    (pad "59" smd rect (at -1.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS_6") (pintype "passive"))
    (pad "60" smd rect (at -1.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VDD_5") (pintype "passive"))
    (pad "61" smd rect (at -2.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "QAn") (pinfunction "TRD1/SQID1/ERXD0/PMD1/RE1") (pintype "passive"))
    (pad "62" smd rect (at -2.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "QBn") (pinfunction "TRD2/SQID2/ERXDV/ECRSDV/AECRSDV/PMD2/RE2") (pintype "passive"))
    (pad "63" smd rect (at -3.25 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "WIFI_RESETn") (pinfunction "TRD3/SQID3/ERXCLK/EREFCLK/RPE3/PMD3/RE3") (pintype "passive"))
    (pad "64" smd rect (at -3.75 -5.738 270) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "WIFI_EN") (pinfunction "AN18/ERXERR/PMD4/RE4") (pintype "passive"))
    (model "PIC32MZ0512EFE064-I_PT.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 178.308 74.168 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1uF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 149.606 91.948)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:228DD1S1AAFAMSC" (layer "F.Cu")
    (tedit 0)
    (at 70.612 114.808 180)
    (descr "228DD1S1AAFAMSC")
    (tags "Switch")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.ctscorp.com/wp-content/uploads/228D.pdf")
    (property "Description" "SWITCH TACTILE SPST-NO 0.05A 12V")
    (property "Footprint_1" "228DD1S1AAFAMSC")
    (property "Height" "6.4")
    (property "Manufacturer_Name" "CTS")
    (property "Manufacturer_Part_Number" "228DD1S1AAFAMSC")
    (property "Mouser Part Number" "774-228DD1S1AAFAMSC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CTS-Electronic-Components/228DD1S1AAFAMSC?qs=BJlw7L4Cy7%252Bx9Gylbq7xIw%3D%3D")
    (property "Reference_1" "S?")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "228DD1S1AAFAMSC")
    (attr through_hole)
    (fp_text reference "S3" (at 1.725 4.572 180) (layer "F.SilkS"))
    (fp_text value "228DD1S1AAFAMSC" (at 1.725 -1.15 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.725 -1.15 180) (layer "F.Fab"))
    (pad "L1" thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 108 "Net-(R23-Pad2)") (pinfunction "A__AMBER") (pintype "passive"))
    (pad "L2" thru_hole circle (at 3.45 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K_AMBER") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 0.125 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 3.325 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH2") (pintype "passive"))
    (pad "S1" thru_hole circle (at 1.15 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 120 "AUTOSTART_TOGGLEn") (pinfunction "COM") (pintype "passive"))
    (pad "S2" thru_hole circle (at 2.3 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "NO") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.514 57.658)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 3.048 0) (layer "F.SilkS"))
    (fp_text value "27" (at 5.334 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C14-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:BZW04-376BRL" (layer "F.Cu")
    (tedit 0)
    (at 106.172 54.61 180)
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "CR1" (at 12.192 1.778) (layer "F.SilkS"))
    (fp_text value "DO-15_6P76X3P53_STM" (at 6.35 3.048) (layer "F.SilkS"))
    (fp_text user "*" (at -1.778 0.762) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "*" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 52 "LOOPa") (pinfunction "CATHODE/ANODE") (pintype "unspecified"))
    (pad "2" thru_hole circle (at 13.7922 0 180) (size 1.651 1.651) (drill 1.143) (layers *.Cu *.Mask)
      (net 16 "Net-(CR1-Pad2)") (pinfunction "CATHODE/ANODE") (pintype "unspecified"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.282 69.85 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.524) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "LOOP_KEY") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(K1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:DIPS1067W107P475L2062H1880Q6N" (layer "F.Cu")
    (tedit 0)
    (at 157.4045 57.15 -90)
    (descr "DIP-6")
    (tags "Transformer")
    (property "Arrow Part Number" "TY-141P")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/ty-141p/triad-magnetics?region=nac")
    (property "Description" "TRIAD MAGNETICS - TY-141P - Audio Transformer, Line Matching, 4 mA, 10 kohm, 10 kohm, Through Hole, TY-14x Series")
    (property "Height" "18.796")
    (property "Manufacturer_Name" "Triad Magnetics")
    (property "Manufacturer_Part_Number" "TY-141P")
    (property "Mouser Part Number" "553-TY141P")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Triad-Magnetics/TY-141P?qs=sK90oOEhQaXZYAU4yeNTTQ%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "T1" (at 16.002 -0.3295) (layer "F.SilkS"))
    (fp_text value "TY-141P" (at 0 0 -90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 59 "AFSK_INa") (pinfunction "PRI_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.75 270) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 60 "unconnected-(T1-Pad2)") (pinfunction "PRI_2") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at 0 9.5 270) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 61 "AFSK_INb") (pinfunction "PRI_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 10.668 9.5 270) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 47 "Net-(C8-Pad1)") (pinfunction "SEC_1") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.668 4.75 270) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 62 "unconnected-(T1-Pad5)") (pinfunction "SEC_2") (pintype "passive+no_connect"))
    (pad "6" thru_hole circle (at 10.668 0 270) (size 2.1 2.1) (drill 1.4) (layers *.Cu *.Mask)
      (net 63 "Net-(T1-Pad6)") (pinfunction "SEC_3") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.304 82.042 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 3.048 0 90) (layer "F.SilkS"))
    (fp_text value "33" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "WIFI_CSn") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.784 65.786 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "33" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(R16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "WIFI_MISO") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 175.514 55.88)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "47pF" (at 6.604 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:100DP1T2B4M7QE_EWI" (layer "F.Cu")
    (tedit 0)
    (at 180.848 95.758)
    (tags "100DP1T2B4M7QE ")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S8" (at 2.413 3.81 unlocked) (layer "F.SilkS"))
    (fp_text value "100DP1T2B4M7QE" (at 2.413 3.81 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.413 3.81 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask)
      (net 126 "unconnected-(S8-Pad1)") (pinfunction "1") (pintype "unspecified+no_connect"))
    (pad "2" thru_hole circle (at 0 3.81) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask)
      (net 125 "+5V") (pinfunction "2") (pintype "unspecified"))
    (pad "3" thru_hole circle (at 0 7.62) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask)
      (net 9 "+5V_SW") (pinfunction "3") (pintype "unspecified"))
    (pad "4" thru_hole circle (at 4.826 0) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask)
      (net 127 "unconnected-(S8-Pad4)") (pinfunction "4") (pintype "unspecified+no_connect"))
    (pad "5" thru_hole circle (at 4.826 3.81) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask)
      (net 125 "+5V") (pinfunction "5") (pintype "unspecified"))
    (pad "6" thru_hole circle (at 4.826 7.62) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask)
      (net 9 "+5V_SW") (pinfunction "6") (pintype "unspecified"))
    (pad "7" thru_hole circle (at -0.127 20.32) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask))
    (pad "8" thru_hole circle (at 4.953 20.32) (size 2.3622 2.3622) (drill 1.8542) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 162.052 51.308 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 50.038 58.42)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "1M" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 88.2885 54.61 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "39" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(CR1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "LOOPb") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 170.434 64.516 90)
    (descr "SSOP, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/40001800C.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SSOP SO")
    (property "Arrow Part Number" "FT231XS-U")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/ft231xs-u/ftdi-chip?region=nac")
    (property "Description" "Full Speed to Handshake USB UART IC")
    (property "Height" "1.753")
    (property "Manufacturer_Name" "FTDI Chip")
    (property "Manufacturer_Part_Number" "FT231XS-U")
    (property "Mouser Part Number" "895-FT231XS-U")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/FTDI/FT231XS-U?qs=Gp1Yz1mis3WFP7tMtj2Z9g%3D%3D")
    (property "Mouser Testing Part Number" "")
    (property "Mouser Testing Price/Stock" "")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -4.55 90) (layer "F.SilkS"))
    (fp_text value "FT231XS-U" (at 0 4.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.5 -2.925 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "unconnected-(U3-Pad1)") (pinfunction "DTR#") (pintype "passive+no_connect"))
    (pad "2" smd roundrect (at -3.5 -2.275 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "U1CTSn") (pinfunction "RTS#") (pintype "passive"))
    (pad "3" smd roundrect (at -3.5 -1.625 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "USB_3V3") (pinfunction "VCCIO") (pintype "passive"))
    (pad "4" smd roundrect (at -3.5 -0.975 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "U1TX") (pinfunction "RXD") (pintype "passive"))
    (pad "5" smd roundrect (at -3.5 -0.325 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "unconnected-(U3-Pad5)") (pinfunction "RI#") (pintype "passive+no_connect"))
    (pad "6" smd roundrect (at -3.5 0.325 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND_1") (pintype "passive"))
    (pad "7" smd roundrect (at -3.5 0.975 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "unconnected-(U3-Pad7)") (pinfunction "DSR#") (pintype "passive+no_connect"))
    (pad "8" smd roundrect (at -3.5 1.625 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "unconnected-(U3-Pad8)") (pinfunction "DCD#") (pintype "passive+no_connect"))
    (pad "9" smd roundrect (at -3.5 2.275 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "U1RTSn") (pinfunction "CTS#") (pintype "passive"))
    (pad "10" smd roundrect (at -3.5 2.925 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "unconnected-(U3-Pad10)") (pinfunction "CBUS2") (pintype "passive+no_connect"))
    (pad "11" smd roundrect (at 3.5 2.925 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R7-Pad1)") (pinfunction "USBDP") (pintype "passive"))
    (pad "12" smd roundrect (at 3.5 2.275 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R6-Pad1)") (pinfunction "USBDM") (pintype "passive"))
    (pad "13" smd roundrect (at 3.5 1.625 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "USB_3V3") (pinfunction "3V3OUT") (pintype "passive"))
    (pad "14" smd roundrect (at 3.5 0.975 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "USB_3V3") (pinfunction "RESET#") (pintype "passive"))
    (pad "15" smd roundrect (at 3.5 0.325 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+5V_SW") (pinfunction "VCC") (pintype "passive"))
    (pad "16" smd roundrect (at 3.5 -0.325 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND_2") (pintype "passive"))
    (pad "17" smd roundrect (at 3.5 -0.975 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "unconnected-(U3-Pad17)") (pinfunction "CBUS1") (pintype "passive+no_connect"))
    (pad "18" smd roundrect (at 3.5 -1.625 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "unconnected-(U3-Pad18)") (pinfunction "CBUS0") (pintype "passive+no_connect"))
    (pad "19" smd roundrect (at 3.5 -2.275 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "PWRENn") (pinfunction "CBUS3") (pintype "passive"))
    (pad "20" smd roundrect (at 3.5 -2.925 90) (size 1.9 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "U1RX") (pinfunction "TXD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-20_5.3x7.2mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 178.308 71.374)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 3.302 -1.016) (layer "F.SilkS"))
    (fp_text value "AP2112K-3.3" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+5V_SW") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "Net-(U5-Pad6)") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "unconnected-(U6-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.812 76.708)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.302 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(C8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.254 77.978)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -2.794 0.254) (layer "F.SilkS"))
    (fp_text value "510k" (at -5.842 0.254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:XDCR_PEC12R-2220F-S0024" (layer "F.Cu")
    (tedit 64420B04)
    (at 161.798 115.316)
    (property "MANUFACTURER" "Bourns")
    (property "MAXIMUM_PACKAGE_HEIGHT" "16.7 mm")
    (property "PARTREV" "07/21")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S7" (at -5.283 -8.701) (layer "F.SilkS"))
    (fp_text value "PEC12R-2220F-S0024" (at 6.147 18.385) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -2.5 -2.5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 87 "ENCODER_SWn") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 -2.5) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "A" thru_hole circle (at -2.5 0) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 123 "QAn") (pinfunction "CHANNEL_A") (pintype "passive"))
    (pad "B" thru_hole circle (at 2.5 0) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 124 "QBn") (pinfunction "CHANNEL_B") (pintype "passive"))
    (pad "C" thru_hole circle (at 0 0) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "COMMON") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.55 -3.5) (size 3.316 6.632) (drill oval 2.3 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.55 -3.5) (size 3.316 6.632) (drill oval 2.3 2.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 118.364 79.502 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.54 0) (layer "F.SilkS"))
    (fp_text value "10k" (at 4.826 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "MCLRn") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 130.556 90.678)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.524) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.812 74.93 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 2.794 0) (layer "F.SilkS"))
    (fp_text value "10k" (at -3.302 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 90.932 103.378 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "KOS_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 64.262 75.184 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C21" (at 3.556 0 90) (layer "F.SilkS"))
    (fp_text value "10nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 62.484 75.184 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C20" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-6_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 89.647 58.176 -90)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "H11AA1" (at 3.81 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(CR1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "LOOPb") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "unconnected-(U4-Pad3)") (pinfunction "NC") (pintype "no_connect"))
    (pad "4" thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "5" thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "LOOP_SENSE") (pintype "passive"))
    (pad "6" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U4-Pad6)") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 117.348 82.296 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.794 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "MCLRn") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "PGED") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "PGEC") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "unconnected-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "unconnected-(J2-Pad7)") (pinfunction "Pin_7") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "IDLEn") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 127.254 74.422 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 2.794 0) (layer "F.SilkS"))
    (fp_text value "1nF" (at 5.08 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C10-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "HhLibrary:228DD1S1AAFAMSC" (layer "F.Cu")
    (tedit 0)
    (at 60.452 114.808 180)
    (descr "228DD1S1AAFAMSC")
    (tags "Switch")
    (property "Arrow Part Number" "")
    (property "Arrow Price/Stock" "")
    (property "Datasheet_1" "https://www.ctscorp.com/wp-content/uploads/228D.pdf")
    (property "Description" "SWITCH TACTILE SPST-NO 0.05A 12V")
    (property "Footprint_1" "228DD1S1AAFAMSC")
    (property "Height" "6.4")
    (property "Manufacturer_Name" "CTS")
    (property "Manufacturer_Part_Number" "228DD1S1AAFAMSC")
    (property "Mouser Part Number" "774-228DD1S1AAFAMSC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CTS-Electronic-Components/228DD1S1AAFAMSC?qs=BJlw7L4Cy7%252Bx9Gylbq7xIw%3D%3D")
    (property "Reference_1" "S?")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "228DD1S1AAFAMSC")
    (attr through_hole)
    (fp_text reference "S2" (at 1.778 4.572 180) (layer "F.SilkS"))
    (fp_text value "228DD1S1AAFAMSC" (at 1.725 -1.15 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 1.725 -1.15 180) (layer "F.Fab"))
    (pad "L1" thru_hole rect (at 0 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 106 "Net-(R22-Pad2)") (pinfunction "A__AMBER") (pintype "passive"))
    (pad "L2" thru_hole circle (at 3.45 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "K_AMBER") (pintype "passive"))
    (pad "MH1" thru_hole circle (at 0.125 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH1") (pintype "passive"))
    (pad "MH2" thru_hole circle (at 3.325 -2.2 180) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "MH2") (pintype "passive"))
    (pad "S1" thru_hole circle (at 1.15 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 117 "SHIFT_TOGGLEn") (pinfunction "COM") (pintype "passive"))
    (pad "S2" thru_hole circle (at 2.3 0 180) (size 0.95 0.95) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "NO") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.452 103.378 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "850_SHIFT_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "Net-(R22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 171.704 55.88 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 3.302 0.508) (layer "F.SilkS"))
    (fp_text value "47pF" (at 6.35 0.508) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 173.482 72.39 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 3.302 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "+5V_SW") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 146.812 73.152 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 2.8945 0) (layer "F.SilkS"))
    (fp_text value "100nF" (at -4.2175 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.092 103.378 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "220" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "TX_LED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 139.954 103.7855 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "DSP_TU.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.43 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 270) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 38 117.862) (end 196 38.862) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_text "AutoStart" (at 68.58 106.68) (layer "F.SilkS"))
  (gr_text "TX" (at 98.806 106.68) (layer "F.SilkS"))
  (gr_text "Shift" (at 58.674 106.68) (layer "F.SilkS"))
  (gr_text "DSP TU\nRev A\nw6iwi.org" (at 74.93 84.074) (layer "F.SilkS"))
  (gr_text "KOS" (at 88.9 106.68) (layer "F.SilkS"))
  (gr_text "MarkHi" (at 48.514 106.68) (layer "F.SilkS"))
  (gr_text "Motor" (at 78.994 106.68) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.738 67.056)
        (xy 59.182 67.056)
        (xy 59.182 63.246)
        (xy 62.738 63.246)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "In1.Cu") (name "GND") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.818 116.84)
        (xy 39.116 116.84)
        (xy 39.116 39.878)
        (xy 194.818 39.878)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "In1.Cu" "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.756 55.88)
        (xy 38.354 55.88)
        (xy 38.354 38.862)
        (xy 79.756 38.862)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "In2.Cu") (name "+3V3") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.818 116.84)
        (xy 39.116 116.84)
        (xy 39.116 39.624)
        (xy 194.818 39.624)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.738 67.056)
        (xy 59.182 67.056)
        (xy 59.182 63.246)
        (xy 62.738 63.246)
      )
    )
  )
)
